SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    Speakers - Type 1	3
2.1.1    Basis of Design Speaker:	3
2.1.2    Minimum Requirements:	3
3    EXECUTION	4
4    APPENDICES	4
4.1    SPECIFIED PRODUCTS	4
4.1.1    Crestron SAROS SB-200-P-B 	4

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	Speakers - Type 1

2.1.1	Basis of Design Speaker:

2.1.1.1	Crestron SAROS SB-200-P-B  

2.1.2	Minimum Requirements:

2.1.2.1	Stereo amplified sound bar speaker 

2.1.2.2	Performance:

2.1.2.2.1	Output Sensitivity: 83 dB SPL at one meter, both channels driven @ 1-W each 

2.1.2.2.2	Frequency Response: Within plus or minus 3 dB from 100 to 20,000 Hz 

2.1.2.2.3	Go to sleep time: 20 Minutes 

2.1.2.2.4	Amplifier Power: 20 Watts per channel, stereo 

2.1.2.2.5	Woofers: (2) 3 inch polypropylene cone with rubber surround 

2.1.2.2.6	Tweeters: (2) 1 inch polyester dome 

2.1.2.2.7	Passive Radiators: (2) 3 x 4-3/8 inch polypropylene  cone with rubber surround 

2.1.2.2.8	Speaker unit power supply shall be equipped for 100-240 Volts AC, 50/60 Hz power

2.1.2.2.8.1	Maximum power: 50 Watts (500mA)  

2.1.2.2.9	Mounting:

2.1.2.2.9.1	Freestanding: surface or shelf 

2.1.2.2.9.2	Wall mount with included bracket   

2.1.2.3	Enclosures: Plastic housing with perforated metal grill 

2.1.2.4	Connectors:

2.1.2.4.1	Balanced Audio: (1) 5-pin terminal block 

2.1.2.4.2	Unbalanced Audio: (2) RCA female      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron SAROS SB-200-P-B