SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    Keypad User Interface	3
2.1.1    Basis of Design Control Module:	3
2.1.2    Keypad UI	3
2.1.3    Functions - The Keypad UI shall include:	3
2.1.4    Communication and Power	3
2.1.5    Physical	3
3    EXECUTION	3
4    APPENDICES	3
4.1    SPECIFIED PRODUCTS	3
4.1.1    Crestron C2N-CBD-P 	3

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	Keypad User Interface

2.1.1	Basis of Design Control Module:
Specifier Note: Please see system drawings or equipment lists for specified model and quantity.
2.1.1.1	Crestron C2N-CBD-P  

2.1.2	Keypad UI

2.1.2.1	Remote Keypad Controls:  Field-configurable remote keypad with auto-adjusting backlight illuminating replaceable, engravable programmable buttons in number indicated, with white LED indicators, configured to fit in standard single-gang box.  

2.1.3	Functions - The Keypad UI shall include:

2.1.3.1	Custom Control UI - control of integrated system components through custom programming or preset configuration of the system control processor by same manufacturer. 

2.1.3.2	System Integration - device shall support controls for compatible integrated AV systems, HVAC and Lighting hardware, and  scheduling and management systems.  

2.1.4	Communication and Power

2.1.4.1	Communication: Wired Network Protocol 

2.1.4.2	Power:  24 VDC integrated with communication cable  

2.1.5	Physical

2.1.5.1	Single gang form factor     

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron C2N-CBD-P